ZMOD4510 Ultra-Low Power Ozone Firmware Documentation |

Data Fields
ulp_o3_results_t Struct Reference

Variables that receive the algorithm outputs. More...

## Data Fields
float | rmox [8]
float | temperature
float | O3_conc_ppb
uint16_t | FAST_AQI
uint16_t | EPA_AQI

## Detailed Description

Variables that receive the algorithm outputs.

## Field Documentation

## ◆ EPA_AQI

uint16_t EPA_AQI

EPA_AQI stands for the Air Quality Index according to the EPA standard based on ozone.

## ◆ FAST_AQI

uint16_t FAST_AQI

FAST_AQI stands for a 1-minute average of the Air Quality Index according to the EPA standard based on ozone

## ◆ O3_conc_ppb

float O3_conc_ppb

O3_conc_ppb stands for the ozone concentration in part-per-billion

## ◆ rmox

float rmox[8]

MOx resistance.

## ◆ temperature

float temperature

Temperature (degC) used for ambient compensation