ZMOD4510 Ultra-Low Power Ozone Firmware Documentation |

Enumerations | Functions
hs4xxx.h File Reference
HSxxxx Sensor API » HS4xxx Sensor API

HS4xxx sensor declarations. More...

Go to the source code of this file.

## Enumerations
enum | HS4xxx_ErrorCodes_t { hteHS4xxxCRCError = 1 }
| Error code definitions specific for the HS4xxx API. More...

## Functions
int | HS4xxx_Init (HSxxxx_t *sensor, Interface_t *hal)
| Initialize the sensor object. More...
int | HS4xxx_ReadID (HSxxxx_t *sensor, uint32_t *id)
| Read the unique sensor ID of the HS4xxx. More...
int | HS4xxx_Measure (HSxxxx_t *sensor, HSxxxx_Results_t *results)
| Perform a temperature/humidity measurement cycle. More...
int | HS4xxx_MeasureHold (HSxxxx_t *sensor, HSxxxx_Results_t *results)
| Perform a temperature/humidity measurement cycle using hold mode. More...
int | HS4xxx_MeasureStart (HSxxxx_t *sensor)
| Start a temperature/humidity measurement cycle in non-hold mode. More...
int | HS4xxx_MeasureRead (HSxxxx_t *sensor, HSxxxx_Results_t *results)
| Read temperature/humidity results in non-hold mode. More...