ZMOD4510 Ultra-Low Power Ozone Firmware Documentation |

Data Fields
ulp_o3_inputs_t Struct Reference

Variables that are needed for algorithm. More...

## Data Fields
uint8_t * | adc_result
float | humidity_pct
float | temperature_degc

## Detailed Description

Variables that are needed for algorithm.

Parameters

  [in] | adc_result | Value from read_adc_result function
  [in] | humidity_pct | relative ambient humidity (%)
  [in] | temperature_degc | ambient temperature (degC)